

11.4.23

**PumaESD Recommended Tools/Supplies**

**PumaESD TOOLS & SUPPLIES** **KIT …………… $ 639.00** *Kit includes the following:*

1. Duct tape
2. Tape. Blue 1.5”
3. Painters paper- brown, 1-roll
4. Mixer paddle 5-gal (spiral-liquids)
5. Mixer paddle 1-gal (spiral-liquids)
6. 5-gal pail
7. Cotton rags
8. Mix n Measure, 1-Quart qty- 4
9. Mix n Measure,  2-Quart qty- 4
10. Spike shoes-plastic, (tighten spikes securely)
11. Roller frame 9” qty-2
12. Roller cover 9” x 3/8” qty- 4 (purdy/wooster)
13. Roller frame, 18” w end caps qty-1
14. Roller cover 3/8” x 18” qty-2, (purdy/wooster)
15. Brushes 2" qty-4
16. Squeegee 18” by Unger (pull)
17. Squeegee flat 18” gray (push or pull)
18. Extension Pole 60"
19. Conductive copper tape (grounding)

**300 SERIES Only** …**Add $ 117.00**

1. Mixer paddle- (egg beater style - grout-mixes)
2. Trowel, flat 4 x12”
3. Roller cover, LOOP/textured 9” qty-3
4. Roller cover, LOOP/textured 18” qty-3

***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*  
Additional Basic Mixing Tools/Supplies required *(not included w/ above tools/supplies).***

1. **Variable Speed DRILL- ½” chuck or hvy duty Mud Mixer (for slurry systems)** (Home Depot or similar)
2. **5 GAL PAILS** Estimated 3 buckets required, for every 1000 sf of area
3. **ACETONE**  (for cleanup of tools)
4. **4 or 6 mil Plastic and rosin paper/cardboard for mixing area.**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**300 SERIES ESD Systems (SLURRY SYSTEMS) *Spread with trowel, cam rake and/or notched squeegee.***

1. **CAM RAKE OR NOTCHED SQUEEGEE** (Spreading the Slurry Coat) For large wide open areas, slurry coat may be spread using a Cam Rake (MidWest Rake Co.) or notched squeegee. The 24” cam rake requires #2 (1/8”) or #3 (3/16”) cams. It spreads the materials without requiring hand troweling in the main areas. Edges/perimeter always require hand troweling.
2. **NOTCHED SQUEEGEES ………………………………………………………………….. $ 25.67  
   1/2” NOTCH (blade/frame)–** applies slurry at 1/8” **3/8” NOTCH (blade/frame)–** applies slurry at 1/16”



1. **SPIKE/Porcupine ROLLER: ……………………………………….….……. $ 95.26** Use for rolling 3/16” to ¼” slurry base coats
2. **MINERAL SPIRITS** *(increase working time of 300/400 series***)** Use only if substrate/materials are out of proper temperature range (70-80 deg F), or you need more working time. (up to 8 oz/unit for 300/400 series urethane concrete mortar/slurry)  
     
    **SQUEEGEES for THIN MIL & HI-BUILD COATINGS  
      
    EZ NOTCHED SQUEEGEE 18” - BLADE only ……………………. $ 25.67   
    MIL SIZES  
    5- 7 (yellow)  
    8-12 (red)  
    15-20 (green)  
    45-50 (orange)  
    50-60 (purple)   
      
    EZ NOTCHED SQUEEGEE 18” - FRAME only..……………… $ 46.70**



**SPIKED SHOES …………………………………………………… $ 39.00** Strap/tape to bottom of feet  
 Allows you to walk in the wet materials.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**PREP TOOLS   
Fits 17” floor buffer machines (**a/k/a FLOOR MAINTAINER, FLOOR MACHINE, SWING MACHINE)

**DUST SKIRT ………………………………………………………………………….… $139.00**Minimize dust, using this skirt that attaches around the base of



floor buffers. Fits all 17-inch floor machines using a velcro   
strip attachment). Features a 1.25-inch inch dust port for

vacuum hose connection.



**REMOVAL TOOL, 16” DIAMABRUSH…………………………………… $849.00**Diamond scraper tool, designed for removal of glue, mastic,   
and 2-3 mil coatings.

Includes 1.5” riser and standard clutch plate.



**PREP TOOL, 16” DIAMABRUSH ……………………………………….. $ 875.00**

**25 grit** diamonddisc shroud

Includes 1.5” riser and standard clutch plate



**FLOOR MACHINE ……………………………………………………..….. $1,567**.00

**17” FLOOR BUFFER MACHINE**  
HawkF0003-17XHD or similar

**ADDITIONAL TOOLS (for LARGER SLURRY PROJECTS)**

**Battery Powered Quartz Blower/Broadcaster** (Dewalt)……………………………………………………$ 985.00

**110v corded, Quartz Blower/Broadcaster** ………………………………………………………….………… $ 840.00

**Gas, Backpack Quartz Blower/Broadcaster**……………………………………………………………………… $ 1,230.00

4.3 hp low emissions 2 stroke engine, 50 lb hopper capacity, 35 ft horizontal reach,   
 800 cfm, 23 lb, 1 gal fuel tank, (use 50:1 pre-mix fuel)

**ESD Anti-Static Floor Supplies**

**3M 701 Megohmmeter** Resistance Test Kit, with Case…………………………………………………… $ 973.00



**Rental Only: …………………..** $198.00   
 *plus freight (includes 1 week)*